Signing out / signing in a Gas Cylinder from the Biomedical Corridor Stores 
Gas stores are open between 10-10.30 

Stopford Stores will not issue gas cylinders unless at least one of the pair moving the cylinder has a valid gas passport certificate and both are wearing the correct personal protective equipment. 
[bookmark: _GoBack]You will have to show your passport to staff. 

Personal protective equipment to include:
Lab coat (own)
EN166 compliant impact resistant safety spectacles (own) 
EN 388:2016 compliant gloves against mechanical risks (can be borrowed from Stopford Stores)
ISO 20345:2011 compliant safety footwear with steel toe caps (can be borrowed from Stopford Stores) 
 
In order to sign out a cylinder you will need the following:   
2 members of staff / students at least one of whom must hold a current gas passport certificate  
Cylinder trolley in good condition 
Pink / green sign out slip 
PPE as specified above 

Borrowing PPE
Safety shoes and gloves can be borrowed from Stores. 
They are available in a range of sizes so ensure you request the correct size. 
Sit down to change 
If you are going to borrow the shoes you must be wearing socks! 

Returning PPE 
If you want your shoes back you need to return the shoes and gloves to Stores. 

Before you hand the shoes back they must be sprayed with sanitiser spray provided 
Wear eye protection, use in a well ventilated area, away from sources of ignition. 
Shake can well before use. Use in a well ventilated area. Hold can upright, 15 to 20cm from object to be sprayed. Two quick spray actions will disinfect/ deodorise. 
Wash hands after using the spray. 

Sign in the PPE to get your shoes returned. 


Sanitiser spray safety information. 
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Hazards 
Extremely flammable aerosol, causes serious eye irritation, may cause drowsiness or dizziness. 
Pressurised container: May burst if heated. 
Toxic to the aquatic life 

Precautions: 
Keep out of reach of children. Keep away from heat, sparks, open flames, hot surfaces. No smoking. Do not spray on an open flame or other ignition source. Do not pierce or burn, even after use. 
Wash hands thoroughly after handling. Use only outdoors or in a well-ventilated area. Wear eye protection, protective gloves. 
IF IN EYES: Rinse cautiously with water for several minutes. Remove contact lenses, if present and easy to do. Continue rinsing. If eye irritation persists: Get medical attention. Store locked up. Protect from sunlight. Do not expose to temperatures exceeding 50 °C/122°F.
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